* + 6-01-140 – Attachment of Communication Company Facilities on PPL Company Poles
    - 6-01-140-B, BA and D - Clarified the clearance from a communication cable to a streetlight drip loop.
    - 6-01-140-A and B – Added primary underground cable to the 30” exception in the Note.
    - 6-01-140-C – Changed wording from Communication Messenger-Mounted Cabinet to Communication Messenger-Mounted Passive Equipment to prevent confusion.
    - Note 1 – Added reference to 6-01-160 for wireless antennas.
    - Note 5 – Added spacing for drilled holes in wood poles. Added language to clarify exceptions for drilling a metal pole.
    - Note 6 – Added “written” approval.
    - New Note 7 – Definition of a Communication Service Drop.
    - Renumbered notes 7 – 42 accordingly to 8 – 43. Changed note numbers is drawings to match.
    - Note 9 (old 8) – Changed the in-span clearance from neutral, multiplex secondary or aerial cable to a communication cable with a bonded messenger to 12 inches per NESC 2017 Rule 235C2b1b exception 1.
    - Note 11j (old 10j) – Added a note about double container cars.
    - Note 16 (old 15) – Moved note about back bolting from note 17 into 16. Added approved “in writing”.
    - Note 17 (old 16) – Added clarification to limit the use of bolt extenders.
    - Note 27 (old 26) – Clarified language on what a cabinet is and removed the term “equipment cases”. Added that approval for exceptions must be granted by PPL in writing.
    - Notes 28 and 29 (old 27 and 28) – removed the word “equipment case” to prevent confusion.
    - Note 36 (old 35) – Added approved “in writing”.
    - Note 38 (old 37) – Added “written” approval.